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e 2024 USBC MASTERS

DISTANCE: LLFEET VOLUME: 33.795mL

RATIO: 1.741 FORWARD: 13.32mL .’.....
DROP BRUSH: 42 FEET REVERSE: 20.475 mL o O
TANKS: FIRE&ICE PUMP:
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‘THIS PATTERN IS DESIGNED FOR:

DUAL CONOITIONING TANKS | REVERSE DROP BRUSH
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