{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["sheet"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":6,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"sheet","index":0,"n_rows":5,"n_cols":11,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,9]],"flags":["formulas_cached_only"]}
["政府采购产品明细表"]
["序号","产品名称","品目名称","采购方式名称","技术参数","数量","计量单位","单价(元)","总金额(元)","进口/国产","是否面向中小微企业"]
[1,"跑步鞋","跑步鞋",null,"鞋的中底使用FlyteFoam、GEL、SpEVA三层特殊缓冲材料，中层GEL材料分别放于脚部受力较大区域，在后脚根外侧的增厚设计。\n下层FlyteFoam 有机纤维混合而成，有回弹性，能够在超负荷的情况下提供限量形变。\n鞋面采用切断式构造，无缝线结合，使用高伸缩性、透气性的网布材料，可以随着脚部的形状伸缩，在鞋子随着动作发生变形时也能发挥卓越的舒适性。\n鞋面材料还做过防泼水处理，同时拥有防污效果。并且加入了吸收、分解臭味源的光消臭材料，拥有优越吸水性和急速扩散性的速干效果。\n脚踝处的低反弹性记忆泡棉，会配合个人的脚型，逐渐调整成舒服合适的形状，提高了脚踝部舒适性。\n天然橡胶混硅砂制成的外底，鞋底表面硅砂颗粒，能发挥出鞋钉的效果，提高抓地力。\n鞋底使用胎痕设计，增强防滑性。",66,null,1200,79200,"国产","是"]
["联系人：",{"$nulls":7},79200]
["联系电话："]