{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":277,"n_cols":7,"rows_kept":277,"cut":false,"hidden":false,"merged":[[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[15,0,17,0],[15,1,17,1],[15,2,17,2],[15,3,17,3],[15,4,17,4],[1,0,2,0],[1,1,2,1],[51,0,54,0],[51,1,54,1],[51,2,54,2],[51,6,54,6],[76,4,78,4],[76,5,78,5],[55,0,56,0],[61,0,65,0],[76,0,78,0],[76,1,78,1],[76,6,78,6],[80,0,83,0],[80,1,83,1],[80,2,83,2],[80,3,83,3],[80,4,83,4],[80,5,83,5],[80,6,83,6],[76,2,78,2],[76,3,78,3],[84,0,94,0],[84,1,94,1],[84,2,94,2],[84,3,94,3],[84,4,94,4],[84,5,94,5],[84,6,94,6],[95,0,105,0],[95,1,105,1],[95,2,105,2],[95,3,105,3],[95,4,105,4],[95,5,105,5],[95,6,105,6],[106,6,113,6],[112,4,113,4],[114,0,118,0],[114,1,118,1],[114,2,118,2],[114,3,118,3],[114,5,118,5],[114,6,118,6],[106,0,113,0],[106,1,113,1],[122,1,129,1],[122,2,129,2],[122,3,129,3],[106,5,113,5],[106,2,113,2],[106,3,113,3],[122,5,129,5],[122,6,129,6],[132,0,133,0],[132,1,133,1],[132,2,133,2],[132,3,133,3],[132,4,133,4],[132,5,133,5],[132,6,133,6],[122,0,129,0],[134,6,135,6],[140,0,143,0],[140,1,143,1],[140,2,143,2],[140,5,143,5],[140,6,143,6],[134,0,135,0],[134,1,135,1],[134,2,135,2],[134,3,135,3],[144,2,148,2],[144,5,148,5],[134,4,135,4],[134,5,135,5],[156,6,159,6],[144,6,148,6],[149,0,155,0],[149,1,155,1],[149,2,155,2],[149,3,155,3],[149,4,155,4],[149,6,155,6],[144,0,148,0],[144,1,148,1],[160,5,163,5],[156,0,159,0],[156,1,159,1],[156,2,159,2],[173,3,175,3],[173,4,175,4],[160,6,163,6],[164,0,172,0],[164,1,172,1],[164,2,172,2],[164,6,172,6],[160,0,163,0],[160,1,163,1],[160,2,163,2],[178,3,181,3],[173,5,175,5],[173,6,175,6],[176,0,177,0],[176,1,177,1],[176,2,177,2],[176,3,177,3],[176,6,177,6],[173,0,175,0],[173,2,175,2],[178,6,181,6],[182,0,186,0],[182,1,186,1],[182,2,186,2],[182,3,186,3],[182,4,186,4],[182,6,186,6],[178,0,181,0],[178,1,181,1],[178,2,181,2],[187,6,188,6],[189,0,191,0],[189,1,191,1],[189,2,191,2],[189,4,191,4],[189,6,191,6],[187,0,188,0],[187,1,188,1],[187,2,188,2],[187,4,188,4],[192,6,202,6],[203,0,222,0],[203,1,222,1],[203,2,222,2],[203,5,222,5],[203,6,222,6],[192,0,202,0],[192,1,202,1],[192,2,202,2],[192,5,202,5],[235,5,252,5],[223,6,227,6],[230,0,234,0],[230,1,234,1],[230,2,234,2],[230,6,234,6],[223,0,227,0],[223,1,227,1],[223,2,227,2],[223,5,227,5],[235,6,252,6],[253,0,258,0],[253,1,258,1],[253,2,258,2],[253,3,258,3],[253,5,258,5],[253,6,258,6],[235,0,252,0],[235,1,252,1],[235,2,252,2],[259,0,265,0],[259,1,265,1],[259,2,265,2],[259,3,265,3],[268,5,270,5],[259,5,265,5],[259,6,265,6],[266,0,267,0],[266,1,267,1],[266,2,267,2],[266,3,267,3],[266,4,267,4],[266,5,267,5],[266,6,267,6],[268,6,270,6],[271,0,272,0],[271,1,272,1],[271,2,272,2],[271,4,272,4],[271,5,272,5],[271,6,272,6],[268,0,270,0],[268,1,270,1],[268,2,270,2],[273,0,274,0],[273,1,274,1],[273,2,274,2],[273,3,274,3],[273,4,274,4],[273,5,274,5],[273,6,274,6],[275,0,276,0],[275,1,276,1],[275,2,276,2],[275,3,276,3],[275,4,276,4],[275,5,276,5],[275,6,276,6]],"flags":["formulas_cached_only"]}
["序号","产品名称","数量","规格","配置要求","功能要求","到货日期"]
[1,"运动心肺功能测试系统",1,"氧分析器:快速顺次法;二氧化碳分析器:快速红外线法;气体采集方法:高速、低阻抗气体混合室（4.2升)法;流量传感器:压差式传感器.","1.气体混合室（4.2升);2.氧、二氧化碳分析器；3.流量传感器;4.心率遥测系统;5.校准气泵;6.标准气体;7.计算机、打印机；8.工作台车。","通气量,摄氧量,二氧化碳排出量,心率,呼吸商,氧脉搏,氧当量,二氧化碳当量等","2005-03-01"]
[]
[2,"COMBI 功率自行车",1," ","最大功率:1500W;高精度电磁涡流感应式负荷装置;RS232接口;耳夹式心率传感器;无氧、有氧测试程序;人工编程功能.","1.具备有氧、无氧测试和训练功能。2.可测量心率;3.可连接计算机.4.可人工编程.","2005-03-01"]
[3,"彩色多普勒超声系统",1,null,"主机、一体化负荷超声心动图软件、3V2C二个、7L3一个探头、彩打、便携式推车、立卧式功率车一台","此产品对运动员的心脏功能、肌肉、软组织拉伤的检测","2005-03-02"]
[4,"平衡测试训练测试系统",1,null,"8岁以上人群专门的平衡训练仪，索尼VGN-X505AP","多个量化指标快速分析，图形实时显示","2005-03-03"]
[5,"骨密度测定仪",1,"OSTEOSPACE全干式超声骨密度检测","X.Y.Z全方位探头定位系统，检测骨密度骨强度、骨质量、骨弹性",null,"2005-03-04"]
[6,"HOLTER",5,"三通道24小时监测心电、精确ST段分析、详细分析报告、〕高速ECG叠加","心电监测数据处理系统",null,"2005-03-05"]
[7,"超声心动专用功率车",1,null,"负荷范围20－999W、负荷精度3％3W、座位调节120－210cm、时间间歇1－99min、血压测量、脉搏测量",null,"2005-03-07"]
[8,"《轻松检验》",1,"单机版",null,null,"2005-03-08"]
[9,"全自动生化分析仪",1,null,null,null,"2005-03-25"]
[10,"CM-1900冰冻切片机",1,null,null,null,"2005-03-26"]
[11,"磨刀机",1,null,null,null,"2005-03-27"]
[12,"Autostainer",1,"免疫组织染色仪",null,null,"2005-03-28"]
[13,"图象显微成象分析仪",1,null,null,null,"2005-03-29"]
[14,"骨密度分析仪",1,null,"能测定全身","1、扇型扫描"]
[{"$nulls":5},"2.可以在仰卧"]
[{"$nulls":5},"位测定脊柱的"]
[15,"健身台阶训练器",3,null,"同一期","同一期",2005.5]
[16,"高性能自行车测功仪",1,null,"带有数据储存.评估软件","能够模拟实战更换传动比",2005.5]
[17,"股四头肌训练器",1,null,null,"坐.卧两用",2005.1]
[18,"按摩治疗床",2,null,"皮革包橡塑板.透气",null,2005.1]
[19,"按摩治疗床",2,null,"皮革包橡塑板.透气",null,2005.1]
[20,"掌上型血糖测定仪",1,"进口","主机一台，中文操作手册一套","可快速进行血糖测定",2004.12]
[21,"多功能心电图机",1,"进口","主机一台（内置打印机），中文操作手册一套，显示器一台，中文心电图管理系统一套","1、标准十二导联；2、打印分辨率：Y轴≥8点/mm X轴≥16点/mm(走纸速度25mm/s)   ≥8点/mm(走纸速度50mm/s)；3、灵敏度：1/4，1/2，1，2，自动；4、频率响应：0.05～100Hz-3dB,150Hz-6dB；5、记录方式：高速热敏打印（热线阵）；6、交流电源：AC220V,50/60Hz；7、直流电源：DC9.6V(充电电池)；8、交流电池：连续使用时间约60分钟（20℃，充满点状态下，6道记录）；9、安装有 LAN接口，易于与其他心电图管理系统相连接；   10、具有子显示器端口，可随意连接子显示器",2004.12]
[22,"血液分析仪",1,"进口","AC仪器主机；电源线；打印机联接线；稀释液管(红色)；溶血素管(白色)；废液管(黑色)；保险丝；操作手册(中、英文)台式电脑；彩色喷墨打印机；原装试剂（2600人份）；中文处理系统","分析参数十九项（含图）;采血量20ul;全中文操作界面;具有条形码阅读功能;具有串口通讯能力;具有L-J质控图功能;可以储存600个样本结果;可以储存800个质控结果;异常结果报警;自由调整参数范围",2004.12]
[23,"半自动生化仪",1,"进口","F-6124主机1台电源线1根；螺丝刀（换灯用）1把；泵管1根；比色池(带吸液管)1个；比色池盖1个；废液瓶1个；打印机1台打印机电源线1根；打印机承载架1个；操作方法空白卡（带套）1个；测量步骤简明指南1本；操作手册（中、英文）1本；台式电脑、打印机1套；中文处理系统1","1、吸光度范围：-0.2-3.5A,吸光度准确度精密度高;2、波长：340、405、495、546、578、623、690nm，可增至12个;3、光源灯：6v/10w卤素灯;4、分辨率：0.001A;5、检测器：硅光电二级管检测;6、显示屏：2*24数字显示;7、键盘：全封闭触摸键盘，20个按键操作简易;8、电脑接口：V24,RS232接口，双向;9、体积，重量：31*35*16cm/4.5kg.;10、电源：100.120.230.240可以转换，50/60HZ±5%",2004.12]
[24,"尿液分析仪",1,"进口","主机1台 电源适配器1个;传送带 2根;试纸条定位器 1个;打印纸托架 2个;热敏打印纸1卷;英文操作手册   1本;中文操作手册1本;台式电脑、打印机1套;中文处理系统1套.","速度快：600样本/小时;采用CCD检测技术;灵敏度可调整;可存储2500个病人和质控结果;可报告定性或半定量结果;可进行尿十项或尿十一项测定",2004.12]
[25,"国产低温离心机",1,"国产",null,"分离血清5000转以上"]
[26,"国产超声波清洗机",1,"国产","主机一台（标配件）","进行试管清洗",2004.12]
[27,"国产干燥箱",1,"国产","主机一台（标配件）","干燥器皿",2004.12]
[28,"国产冰箱、冰柜","各1台","国产","三开门(290立升冰箱);200立升冰柜","储存冷冻血样及试剂",2004.12]
[29,"激光无痛指血仪",1,"国产","主机一台（标配件）","快速无痛采指血",2004.12]
[30,"精密移液器（10-100微升、200-1000微升可调）","各3","进口",null,"可进行微量试剂的定量移取，用量可调，可进行半支高温消毒。",2004.12]
[31,"全身肌力测试系统",1,"进口","1、5个肌力测试仪（躯干、劲部、腿部、拉力、握力）；2、功率放大及显示器一台（4个接口）；3、电脑测量及分析软件一套（含电脑、打印机）。","1、可进行五种肌力测试；2、实时显示，可同时连接4个测试仪。",2005.3]
[32,"低频治疗仪",1,"进口","主机1台、电源线1条、治疗头4个","2通道输出；带负压按摩电极；25种疾病治疗程式；80个疗程记忆功能；液晶体显示面板；共6种不同的中频治疗方法","2004.12～2005.1"]
[33,"中频(干扰电)治疗仪 ",1,"进口","主机1台、电源线1条、治疗头4个","2通道输出；带负压按摩电极；35种疾病治疗程式；80个疗程记忆功能；液晶体显示面板；共9种不同的中频治疗方法","2004.12～2005.2"]
[34,"双频超声波治疗仪 ",2,"进口","双频37.5mm Ø探头PR-700L x 1;双频16.0mmØ探头-PR-700S x 1;超声支架HH-700 x 1;导电凝胶UG-260GT(260ml)x 1;导电凝胶UG-260GT(260ml)x 1","1.双频率选择;2.可进行不同部位运动伤的治疗","2004.12～2005.3"]
[35,"大功率短波治疗仪",1,"进口","主机一台；13cm、8.5cm、4.2cm电容导子各一付；支架一付；包括大、中、小三种探头式电容导子各一套","频率：27.12MHz；连续和脉冲两种治疗模式；最大输出功率200W连续，400W脉冲；。高屏蔽性能，对周围环境无影响。","2004.12～2005.4"]
[36,"短波治疗仪 ",2,"进口","探头活动臂杆x 1；电感导子70mmØ x1；电容板状导子 x 1；电感板状导子 x 1；绑带 x 1；绑带 x 1；（配各型号导子各一套）","促进深部组织器官的血液循环，增强代谢；降低感觉神经的兴奋性，降低肌肉和结缔组织张力，增加免疫功能；具有解痉，镇痛，消炎，改善血液循环等治疗作用。","2004.12～2005.5"]
[37,"磁振热治疗仪",1,"进口","MS超强磁力导子x2；ES超强肩/膝导子x1；N颈部导子x1；导子套x2；检磁器x1；电源线x1；台车x1。","镇痛，镇静，降压，消炎与消肿，软化疤痕与松解粘连，促进骨痂生长。适用于各种骨关节疾病、颈腰椎疾病各种慢性无菌性炎症。",2005.3]
[38,"双人牵引装置  ",1,"进口","主机x1；床x1(加长至2米)；椅子x1；骨盆绑带x1；颈部绑带x1；腋下绑带x1；骨盆延伸棒x1；颈部延伸棒x1；骨盆温热导子x1；颈部温热导子x1；患者遥控器x2。","可同时对两个人进行颈椎或腰椎牵引。主要治疗椎间盘突出症，也可用于脊柱矫正，与上述的磁疗设备配合使用效果更佳。",2005.3]
[39,"全日康治疗仪",6,"国产","主机一台（标配件）,导连线一套","可促进血液循环",2005.8]
[40,"中频治疗仪",6,"国产","主机一台（标配件）,导连线一套","可促进血液循环",2005.8]
[41,"TDP（神灯）治疗仪",4,"国产",null,"消炎止痛",2005.8]
[42,"森林浴(包括负氧离子发生器，纯氧激活机；视听系统)",1,null,"１.负氧离子发生器；　　　　　　　　２纯氧激活机；　　　　　　　　　　３视听系统；                    4、森林浴系统；5、16人座装置。","16人座，恢复疲劳，吸氧、娱乐（视频、音响）、蒸浴等",2005.12]
[43,"智能模拟按摩治疗床",1,"日本产","按摩床（标配件）","应用CEL滚动动作模拟人工推拿的智能理疗床。其独特之处在于脚部的推拿按摩治疗，新开发出的偏中心位相差滚动，能对脚部进行夹压按摩及交替指压，达到推拿的治疗效果。本机器装有英特尔的计算控制器（CPU），使它在指压、按揉、振动、腰部、颈部的5种分类基础上组合出14种全身治疗方法和11种局部定点治疗方法，共25种治疗方法。配合远红外线温热疗法。",2005.8]
[44,"无线遥控按摩椅",6,"台湾产，进口","220V/50Hz;无线遥控；","本机器装有英特尔的计算控制器（CPU），使它在指压、按揉、振动、腰部、颈部的5种分类基础上组合出14种全身治疗方法和11种局部定点治疗方法，共25种治疗方法。配合远红外线温热疗法。","2005.3(进2台) 2005.8(进4台)"]
[45,"便携式X光机",1,"SDx0.1-0.5/75(国产)","透视.摄片；配有快速自动洗片机","图象清晰．分辨率高,可进行透视.照片.",2005.3]
[46,"针灸治疗仪",2,"国产","治疗仪1台;电源线1根;输出连接线1套","交流／直流电均可用；用于软组织伤的治疗",2005.3]
[47,"高压消毒锅",2,"国产","主机（标配件）","可进行高温、高压消毒，压力：1.4--1.65公斤/平方厘米",2004.12]
[48,"紫外灯",1,"灯管波长253。7/360mm","具备紫外灯的功能",null,2005.2]
[null,null,null,"定时器1-30分"]
[null,null,null,"耗电20VA"]
[null,null,null,"灯头调节90mm"]
[49,"血球分析仪",1,"日本POCH-100I3分类","备墨，各种液体",null,2005.2]
[null,null,null,"血球记数仪"]
[50,"腹肌练习器",1,"96cm/80cm/115cm",null,null,2005.2]
[51,"卧式大腿下压练习器",1,"115cm/79cm/96cm",null,null,2005.2]
[52,"大腿内外侧肌练习器",1,"125cm/65cm/130cm",null,null,2005.2]
[53,"共振分析仪",1,null,null,null,2005.2]
[54,"半自动生化分析仪",1,"记忆量：",null,"能准确测量",2005.2]
[null,null,null,"100个实验参数",null,"各种生化指标"]
[null,null,null,"200个病人结果"]
[null,null,null,"1024个质检结果"]
[null,null,null,"分辨率：A=0.001"]
[55,"芬兰MK-3酶标仪",1,null,null,null,2005.2]
[56,"血球分析仪",1,"三分类",null,null,2005.2]
[57,"可调 移液器",1,"0.5-10ul",null,null,2005.2]
[58,"可调 移液器",1,"40-200ul",null,null,2005.2]
[59,"可调 移液器",1,"200-1000ul",null,null,2005.2]
[60,"可调 移液器",1,"5-40ul",null,null,2005.2]
[61,"连续式移液器",1,"10-5000ul",null,null,2005.2]
[62,"坐式转体练习器",1,"86cm/75cm/135cm",null,null,2005.2]
[63,"坐式下斜蹬腿练习器",1,"145cm/85cm/126cm",null,null,2005.2]
[64,"提踵练习器",1,"105cm/65cm/165cm",null,null,2005.2]
[65,"身体成分分析仪",1,null,"主机：手提式，便携，内置充电电池及打印机电极导线：4通道电极充电器：为内置电池充电","以人体电阻为基数，测量身体脂肪、水分、瘦体重比例，各部分的相对重量，基础代谢量。3分钟完成测试，屏幕操作提示，使用方便。","60天"]
[]
[]
[66,"身体成分分析仪专用电极","5包",null,null,"配合BI-310主机使用","60天"]
[67,"桑拿房",2,null,"房体：4米*4米*210  桑拿炉：FLA260      控制器：FALA4PK","人体在桑拿房中，通过湿度低、温度高环境的熏蒸，汗液很快的流出以驱除体内的废物，同时能促进体内的血液循环和心血管的弹性。","45天"]
[]
[]
[]
[68,"热水按摩池",2,"8立方米","高压按摩水泵：2HP 1台     过滤水泵：1 HP 1台     高压按摩喷头：6个过滤砂缸连石英砂 1套     电热保温炉：24KW  1台     自动消毒器：1套  池低灯连变压器： 4 套    注/入水器：4个  主排水器：1个 沟道满水器：2个","热水按摩池的温度一般在36度至38度，经过泡浴和按摩喷嘴的水力按摩，可以起到放松身体和疗伤的作用。尤其是对腰背及小腿酸痛的人效果更好。 ","45天"]
{"$rows_empty":10}
[69,"暖水按摩池",2,"14立方米","高压按摩水泵：2HP 2台     过滤水泵：2 HP 1台     高压按摩喷头： 14个      过滤砂缸连石英砂 1套     电热保温炉：54KW  1台     自动消毒器：1套 池低灯连变压器： 8 套    注/入水器：8个主排水器：1个      沟道满水器：4个","作用与热水池相同，只是水温为34度至36度。更适合于大多数人。","45天"]
{"$rows_empty":10}
[70,"冷水按摩池",2,"8立方米","过滤水泵： 1HP 1台","自来水水温，配以过滤和消毒系统。冷水池是配合桑拿房蒸汽房及热、暖水池使用，使肌体通过几次冷热的循环刺激，使人体的毛孔经过几次张开和闭合，起到排泄废物和增强体质的作用。","45天"]
[{"$nulls":4},"过滤砂缸连石英砂 1套"]
[{"$nulls":4},"自动消毒器：1套"]
[{"$nulls":4},"池低灯连变压器： 4 套"]
[{"$nulls":4},"注/入水器：4个"]
[{"$nulls":4},"主排水器：1个"]
[{"$nulls":4},"沟道满水器：2个"]
[]
[71,"药浴木桶",12,null,"尺寸：1450MM*700MM*800MM","香柏木香熏木桶是传统舒适的泡浴方式，可迅速消除疲劳，放入不同配方的中草药，可起到不同的疗伤和治疗慢性病的作用。特别是对关节酸痛有特别好的疗效。","45天"]
[{"$nulls":4},"配置：双座板，双头靠，下水软管"]
[{"$nulls":4},"香柏木制造"]
[{"$nulls":4},"单人使用"]
[{"$nulls":4},"药浴功能"]
[72,"全血分析仪",1]
[73,"尿液分析仪",1]
[74,"超声心动仪",1]
[75,"多方位震动力量训练仪",2,null,"2个二维震动平台","采用不同的震动频率,刺激大小机群,使运动员更多肌肉参与训练的主要机器，对提高运动成绩有很大作用","100天"]
[{"$nulls":4},"3个连续可变的角度"]
[{"$nulls":4},"交互震动顺序随机性"]
[{"$nulls":4},"2个侧扶手"]
[{"$nulls":4},"多功能控制板（可平滑的调节震动频率0.5-12.5HZ）"]
[{"$nulls":4},"5分钟自动停机功能"]
[{"$nulls":4},"尺寸：1000MM*810MM*1300MM"]
[{"$nulls":4},"重量：120KG"]
[76,"运动手表",10,null,null,null,"100天"]
[77,"液压等动训练仪","1套"]
[78,"DITY 双通道动态电流和TENS治疗仪",2]
[]
[79,"TNS双通道TENS治疗仪",2,null,null,null,"60天"]
[]
[80,"牵引床",1]
[81,"牵引器",1]
[82,"按摩椅（大号）",10]
[83,"按摩器",20]
[84,"E-Star Plus免疫原分析仪","1台","1. 光学系统： 8个测试通道，405 nm－690 nm频宽。","1.  全中文windows操作系统下运行。","运动员常见免疫问题诊断与分析。","2005年3月到货。"]
[null,null,null,"2.  滤光片： 6个。","2.  兼酶标功能。"]
[null,"(美国Cowealth Med)",null,"3.  光源： 12v/20W卤光灯。","3.  独立试剂分配。"]
[{"$nulls":4},"4.  自带清洗装置。"]
[85,"跑台","1台","1.  速度：44 Km/h。","1.  有保护装置。","运动员心肺功能诊断与分析。","2005年3月到货。"]
[null,"(德国JAEGER)",null,"2.  坡度：0-25%。","2.  与Oxycon Pro系统兼容。"]
[null,null,null,"3.  皮带面积："]
[null,null,null,"163 ×63 cm。"]
[null,null,null,"4.  功率：2.2 KW。"]
[86,"低氧高温高湿训练系统","1套","达到功能要求。","空气压缩机、分子膜、CO2和O2传感器、各种控制电子阀均为国际著名品牌产品。","全自动控制；","2005年3月完成。"]
[null,"（CNRO）",null,null,null,"模拟海拔高度0-6000米；氧浓度范围10-20%；"]
[{"$nulls":5},"最高温度40℃；"]
[{"$nulls":5},"最大湿度90%；"]
[{"$nulls":5},"低氧供给容积120立方米在2小时达到预定低氧程度；"]
[{"$nulls":5},"氧浓度误差±1%；"]
[{"$nulls":5},"最大噪音<70dB；CO2<5000 ppm。"]
[87,"训练跑台","2台","长：1000 mm","电刺激开关，刺激电压50-400V；","五条跑道，每条宽85mm，高120mm；","2005年4月到货。"]
[null,"（国产段氏）",null,"宽：560 mm","红外线控制发光、发声。","跑速无级可调，范围0-70m/min；"]
[null,null,null,"高：350 mm",null,"使用电压220v单向，频率50Hz，共功率200w。"]
[null,null,null,"重：35 Kg"]
[88,"身体成份分析仪","1台","深度：1320 mm","测试仓；","利用空气置换原理测试人体脂肪重量、体重、脂肪比重、瘦体重。","2005年3月到货。"]
[null,"（美国BOD POD）",null,"宽：890 mm","测试控制台；"]
[null,null,null,"高：1550 mm","体重称；"]
[null,null,null,"仓体容积：450 L","自动校准系统。"]
[89,"全自动生化分析仪","1台","1450×780×1210 mm；重420 kg；","主机标准配置；","恒速400测试/小时；","2005年3月到货。"]
[null,"（日本OLYMPUS）",null,"测量波长340-800 nm，固定13种波长，单/双波长测定，有380 nm,精度±2 nm。","配备UPS、自动纯化水系统。","同步分析最大51项；"]
[{"$nulls":5},"终点法、速率法、固定时间法、电极法；"]
[{"$nulls":5},"连续进样，自动重测；"]
[{"$nulls":5},"常规同时80份样品；"]
[{"$nulls":5},"样品量范围2.0-50 ul；"]
[{"$nulls":5},"可使用国产或进口试剂；"]
[{"$nulls":5},"比色杯可终身使用；"]
[{"$nulls":5},"具有自动重检和远程诊断功能。"]
[90,"运动员机能","1套","标准。","标准系统配置。","无创性评价运动员承受训练负荷反应和机能诊断，可评价运动员的神经系统、能量系统、心肺功能等的变化。","2005年3月到货。"]
[null,"诊断系统"]
[]
[91,"信息检测仪","1台","标准便携式。","设备标准配置；","可进行一般健康检查； 营养素检查；","2005年3月到货。"]
[null,"（国产SAMECOM）",null,null,"全套软件包（可检测1898项指标）。","骨质疏松检查； 亚健康检测。"]
[92,"半自动生化分析仪","1台","620×330×320","流动式32 ul不锈钢比色池，钨灯光源；","波长340-900 nm；","2005年3月到货。"]
[null,"（美国MD）",null,null,"滤光片340, 405, 550, 546, 578, 630。","精度±2 nm；"]
[{"$nulls":5},"光径1 cm；"]
[{"$nulls":5},"温度设定：室温、25℃、30℃、37℃。"]
[93,"低速自动平衡离心机","2台","460×370×440","一号水平转子：7ml×10×4、10 ml×7×4、150 ml×4。","自动平衡<15 g；","2005年3月到货。"]
[null,"（河北白杨离心机）",null,null,null,"快速停机小于30秒；"]
[{"$nulls":5},"加速小于15秒；"]
[{"$nulls":5},"最高转速5000转/分；"]
[{"$nulls":5},"交流半频；无碳刷电机。"]
[94,"电热恒温水箱","1台","水槽容积","标准","温度范围37-65℃；","2005年3月到货。"]
[null,"（北京）",null,"600×300×150 cm",null,"温度波动±0.5℃；"]
[95,"台式数控超声波清洗机","2台","610×410×380；","标准","温度可调20-80℃；","2005年3月到货。"]
[null,"（舒美牌）",null,"容积27 L。",null,"功率可调40-100%；"]
[{"$nulls":5},"时间可调1-480 min。"]
[96,"高速数字摄像系统","1套","速度：可调，高至5000Hz","高速数字摄像机2台","对高水平运动员进行真正的高速录像，从而实现其微观定量技术诊断和微观定性技术分析及显示。","2005年3月到货。"]
[null,null,null,"分辨率：最高达1280×1024","专用图像采集卡及特配硬件1套"]
[null,null,null,"曝光时间：1微秒至24毫秒","专用录像采集软件1套"]
[null,null,null,"控制双（Dual）数字录像机，高速传输数据进入特置硬盘（长时间摄像）","软件开发工具1套"]
[null,null,null,"镜头：Nikkon 35-200","镜头2个"]
[null,null,null,"专用电缆：配套20米","专用电缆2条"]
[null,null,null,"专用电源电缆：5米","专用电源电缆2条"]
[null,null,null,"专配计算机：P4, 1GB, 120GB","专配计算机1台"]
[null,null,null,"Manfrotto","三角架2个"]
[{"$nulls":4},"系统配件（直流电源、接口、导线、辅助硬盘等）"]
[{"$nulls":4},"系统集成、安装和培训"]
[97,"Noraxon - Telemyo2400T/PC - 16 Channel 肌电测试系统","1套","Telemyo 2400T","16-Channel Radio- Frequency Telemetry EMG Transmitter, consists of :","对人体肌群的肌电信号进行遥测，通过所测信号揭示肌肉发力的特点和时序，评价肌肉力量特征和神经支配模式。此系统可与运动分析系统、测力分析系统同步测试。","2005年3月到货。"]
[null,null,null,"Telemyo 2400R","Telemyo carrying case"]
[null,null,null,"MyoResearcn","Telemyo transmitter×2"]
[null,null,null,"NorAngle II","PC-card radio receiver"]
[null,null,null,"NorSwitsch II","Transmitter carrying pouch"]
[{"$nulls":4},"16 set of electrode cables"]
[]
[{"$nulls":4},"16-Channel Radio- Frequency Telemetry EMG Receiver"]
[]
[{"$nulls":4},"PCMCIA无线信号接受卡"]
[]
[{"$nulls":4},"数据采集分析软件Data acquisition and extensive analysis software, including: protocols function, report writing capabilities and so on"]
[{"$nulls":4},"MyoVideo"]
[{"$nulls":4},"数据采集及图像信号同步软件Video and EMG acquisition and Sychronization"]
[]
[{"$nulls":4},"关节角度传感器Electrogoniometer, 2×2-axis"]
[]
[{"$nulls":4},"开关传感器Foot Strike System, Four Sensors per foot"]
[{"$nulls":4},"系统配件"]
[{"$nulls":4},"培训"]
[98,"GTS-602/OP型影像测量标定全站仪","1套","全套","主机＋软件","在大范围运动项目的运动技术研究中，可精确地测量空间三维座标点位置。","2005年2月到货。"]
[null,"（日本）",null,"大内存","叁棱镜各1套"]
[null,null,null,"DOS系统","木脚架1套"]
[null,null,null,"PC卡","铝脚架1套"]
[{"$nulls":4},"配件"]
[99,"三维测力平台支架","4个","请工厂测量并定做。","公差小于0.01 mm。","垂直与水平。","2005年2月完成。"]
[100,"三维测力平台木制盖板","3个","请工厂测量并定做。","烘干、不变形。","垂直与水平。","2005年2月完成。"]
[101,"多方位振动力量训练仪","1套","上下振动，","标准振动仪，","用于运动员振动力量训练与实验，","2005年4月到货。"]
[null,"（德国 SCISENS 公司）",null,"前后振动，","视觉手动控制板，","用于运动员协调能力训练与实验。"]
[null,null,null,"左右振动，","配件。"]
[null,null,null,"振幅可调，"]
[null,null,null,"振频可调。"]
[102,"2米高频测试平板系统","1套","2米高频测试平板系统","3D Box （介面盒）","简便地在训练现场、实验室等进行动力学测量与分析，并可进行力量和技术诊断。","2005年3月到货。"]
[null,null,null,"长×宽×高（毫米）：","3D Box-Plate连接线"]
[null,null,null,"2070×460×20","2 Meter Plate （2米高频测试平板）"]
[null,null,null,"有效测试面积：","Scientific Software （最新科研用软件）"]
[null,null,null,"1952×325","Notebook （说明书）"]
[null,null,null,"采样频率：","SCSI Card (SCSI卡)"]
[null,null,null,"300－500 Hz","SCSI Cable (SCSI连接线)"]
[null,null,null,"传感器数量：","赠送 0.5 Meter Plate （0.5米高频测试平板）"]
[null,null,null,16384,"培训"]
[null,null,null,"质量（千克）："]
[null,null,null,21]
[null,null,null,"测试范围:"]
[null,null,null,"0.25-125 N/cm2"]
[null,null,null,"（可根据需求提高量程）"]
[null,null,null,"操作系统："]
[null,null,null,"Windows"]
[null,null,null,"精度：3.3%"]
[null,null,null,"重复误差：<0..98"]
[103,"HRInstant心率实时监测系统","1套","同时实时监测7个运动员训练时的心率。","多通道心率实时监测软件－HRInstant中文版 1套。","用于各种室内外项目训练的心率实时监测，帮助教练员实时监测运动员的训练负荷和体能状态。","2005年3月到货。"]
[{"$nulls":4},"心率信号采集器PL-T31REC 7套。"]
[{"$nulls":4},"心率数据发射器ST-HP100HR 7个。"]
[{"$nulls":4},"心率数据接收器ST-BTHR 1个。"]
[{"$nulls":4},"充电器、电缆等配件 1套。"]
[{"$nulls":4},"安装和培训。"]
[104,"行为记录分析系统（Oberver）","1套","行为采集分析软件和现场行为标记仪。","行为采集分析软件","数据采集、分析和现场标记。","2005年3月到货。"]
[{"$nulls":4},"(observer Video-Pro"]
[{"$nulls":4}," software)；"]
[{"$nulls":4},"信号压缩卡"]
[{"$nulls":4},"(MPEG-encoder boards)；"]
[{"$nulls":4},"现场行为标记仪"]
[{"$nulls":4},"(Observer Mobile)。"]
[105,"生物反馈训练仪","1套","蓝牙技术10通道16个参数生物反馈系统","蓝牙技术10通道16个参数生物反馈系统",null,"2005年3月到货。"]
[]
[106,"眼动无限发射系统","1套","IV-PCP-12-X: ","IV-PCP-12-X:","以最高250 hz的频率捕捉眼部的高级活动。","2005年3月到货。"]
[null,"（Smi）",null,"Portable lunchbox PC ","Portable lunchbox PC "]
[null,null,null,"Wireless option","Wireless option"]
[107,"动态脑电图仪","1套","放大器：Solor rover",null,"常见脑电图回放、测量，地形图功能、功率谱，正常人参照值，比值检验等。","2005年3月到货。"]
[null,"（Solar）",null,"软件：Solor 2000"]
[108,"行为观测监控摄录系统","1套","松下产品，外带高清晰度录像机JVC，DVCOM数码录像机Sony球形摄像头等设备。","行为观测监控系统需要根据实验室环境和功能进行开发和设计，因此具体配置要求需要跟公司讨论和才能运行。","记录团体交流互动咨询和心理模拟训练过程。在实验对象同意的情况下记录整个心理咨询和训练过程。","2005年5月到货。"]
[null,"（松下）"]
[109,"多人心理训练中央控制系统","1个","有线中央站CTU，4人同步反馈心理训练中心。","需要与公司共同开发确定配置。","同时进行团队心理训练。","2005年5月到货。"]
[null,"（Spirit）"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}